###############################################################
# bochsrc.txt file for DLX Linux disk image.
###############################################################

# how much memory the emulated machine will have
megs: 32

# filename of ROM images
romimage: file=../BIOS-bochs-latest, address=0xf0000
vgaromimage: ../VGABIOS-elpin-2.40

# what disk images will be used 
floppya: 1_44=floppya.img, status=inserted
floppyb: 1_44=floppyb.img, status=inserted
diskc: file=hd10meg.img, cyl=306, heads=4, spt=17
newharddrivesupport: enabled=1

# choose the boot disk.
boot: c

# where do we send log messages?
log: bochsout.txt

# disable the mouse, since DLX is text only
mouse: enabled=0
